Purpose of step two is controlling interrupts over I/O devices. I/O devices cannot send that frequent interrupts to CPU. So we need something to say that has input from your device to CPU. Step2 takes the interrupt signal from device and sends to CPU. At the end, CPU no need to wait that slow I/O devices and can compute with own speed properly.