Context switch is the thing that saves all registers, memory, sequence of instructions and switch it to another program. For instance, program A on its 100th instruction and CPU wants to run program B it actually freeze it and continue to start at 100th instruction. Here has at least 2 context switches program A-B and program B-A. Also user to kernel mode or kernel to user mode is a context switch.