If its a TLB hit then it takes it from cache. If not goes to main memory. If its TLB hit but cache miss it again goes main memory.

Avg = (1 + 2) \* 0.99 \* 0.99 + (1 + 30) \* 0.99 \* 0.01 + (30) \* 0.01

As its not mentioned I assumed TLB miss as 30 clock cycle too.