Interrupt driving is not controlling I/O device like programmed I/O. Instead, only take care interrupts only interrupt arrives. Polling is quite same but doing it by blocking while handling it in background. CPU again do his job in a software support while interrupt driven is hardware support.